# Legend

Color codes define connectivity status or work order status for each port on every panel, scanner or work area outlet.

Scanner Ports Scanner port colors define the status of any given connection of the back of the scanner. Conditions include: unused ports, unconfigured connected panels, configured panels missing, configured panels, scanned panels, and panel connection work orders.
Panel Ports
Panel port colors define the status of patch cord connections between ports. Conditions include: unused ports, ports missing patch cords, unplanned or rogue patch cords, mixed connections, current work orders, and past due work orders.
Switch Ports
Switch ports colors define the status of user defined connections to a switch. Conditions include: unused ports and ports assigned to a panel.
Work Area Outlets
Work area outlet colors define the status of a channel and/or device connections to that outlet. Conditions include: outlets not assigned to a patch panel, outlets assigned to a patch panel, outlets with a terminator, outlet connected to a single device, or an outlet that is part of a full channel.
Channel
Channel status represents connectivity between layer 1 components using color and line style. Conditions include: confirmed connections, inferred connections, and partial channels.

Click here for the legend