# Panel Attributes

| Name

- Name that is represented next to the icon in the site tree

Type

- Defaults to "Panel"

U Position

- Panel "U-location" - drop down box shows available positions

Asset Tag

- Asset tag information

Number of ports

- Defaulted to selected value

Panel Type

- Select: PP or CC
- PP - Patch panel for horizontal cables for both cross connect and interconnect applications
- CC - Crossconnect panel for connection to a switch in cross connect applications

Panel HW Type

- Defines the hardware type of the panel
- Select: Copper, Optical, Undefined
- Select copper or optical before attaching to the scanner.

Connection Type

- Select: Crossconnect or Interconnect
- Defines default panel operation for PP type panels.

Model Number

- Reserved for future use