# Outlet Attributes

| Name Name that is represented next to the icon in the site tree Type Defaults to "Outlet" X
Device icon label "x-coordinate" pixel position
Y
Device icon "y-coordinate" pixel position
Status
Reports the status of the outlet. (unconnected, outlet, partial channel, full channel)
Cable Type
Patch cable type connecting device to work area outlet. (C5e, C6, C6A, etc.)
Cable Color
Horizontal cable color connecting work area outlet to the panel.
Cable Length
Horizontal cable length connecting the work area outlet to the panel.
Description
Field for user assigned information.
Security Level
User defined options: Undefined, Low, Medium, High. Used to define the importance of the outlet status changes. Security level is included in alarm information.
Marked Number
The number on the outlet faceplate.
Enabled
True - Scan outlet
False - Bypass outlet scan
MAC
MAC address of device attached to the outlet.
IP
IP address of the device attached to the outlet.