# Fiber Panel

The fiber patch panels are self contained and powered directly from the scanner. The right side “StatB” LED indicates either “Panel Guidance” or “”Panel Power”. The left side “StatA” LED indicates panel polling. Each patch panel mounts in any standard 19” rack. Each panel is connected to a scanner using standard Cat5e or better patch cords.

In addition, the fiber patch panel includes fiber slack management in a sliding drawer configuration.

Front View 1 - Patch panel - shown with and without port dust covers 2- Slack Drawer Drawer slides open to reveal slack manager. Patch cables plugged into port 23 and port 24, both internally and externally. 3 - Panels in rack
Similar to the copper panels, each port LEDs provides guidance to the patch cords of interest.
a) When “Stat B” turns red, this indicates a port on the panel requires attention
b) The port LED indicates the port requiring attention (i.e. add or remove a patch cord)
4- Patch Cables
Fiber patch cables are available in as “Dual LC” in both multimode and single mode.