# Patching - Racks

Note: Patching requires the PP panel selected is attached to a scanner

### Add patch (video)

Edit Mode = On WO Mode = On |
Left Click - Select empty port Next, using the right mouse button: Drag and drop port from PP to CC (or CC to PP) or Drag and drop port from PP to Switch
Fill in work order parameters Click "Submit" |

### Remove Patch (video)

Edit Mode = On WO Mode = Off |
Select port with patch cord |
Left Click - Select "Disconnect Patch Cord" |
Fill in work order parameters Click "Submit" |