# Network Settings

1 - Scanner Menu - After logging in, select "Configuration > Network" 2- Enable DHCP Checked: Scanner uses DHCP to configure network parameters Not Checked: Scanner uses user defined network parameters 3 - Domain name - Network domain name used for scanner to server communications. Assigned automatically by DHCP or manually by user.
4 - User defined network parameters - These values are not used if EnableDHCP is checked
Default Gateway - Default communication gateway
Subnet Mask - Scanner subnet mask setting
IPAddress - Scanner network IP address
5 - DHCPnetwork parameters - These values are used if EnableDHCP is checked. This values are automatically populated and can not be changed by the user.
DHCPIPAddress - Scanner network IP address
DHCPSubnet Mask - Scanner subnet mask setting
DHCP Default Gateway - Default communication gateway
DHCPServer - The DHCP server from which the MIIM scanner acquired networking IP address configuration
6 - Options
Apply - Commits changes to the scanner configuration
Clear - Reverts back to previous settings
Renew IP Address - Scanner renews IP address from DHCP server