# Virtual Panel

### Front View

Clicking on the left-most or right-most areas of the panel toggles between front and rear view of the panel.
Panels with yellow outlines for ports and labels represent optical panels.
Panels with gray outlines for ports and labels represent copper panels.
The light on the far right indicates status of panel to scanner connectivity.

- Green - Panel connected to scanner; actively scanning
- Yellow - Panel assigned to scanner, not scanning
- Red - Panel to scanner communications broken
- Black - Panel not associated with scanner

Port color description, click here.
A "right-click" on the panel displays a menu. The menu has the following options:
Delete - Delete panel from rack
Change Position - Changes panel position in the rack
Confirm panel patch cords - Confirms all non-designed (red) patch cords as a part of the design (green)
Disattach scanner port - Removes panel association from scanner port

### Rear View

Clicking on the left-most or right-most areas of the panel toggles between front and rear view of the panel.
The port color indicates assignment of panel connectivity:

- Green - PP Panel: Panel port is assigned to a work area outlet
- Green - CC Panel: Panel port is assigned to a switch
- Black - Panel port is not associated